Installation

1. Place the included lds file into the "downloads" folder of your Level-D 767 Winglet expansion.

2. Open the Level- D 767 repaing manager in the same folder, select "ADD REPAINT(S)" and then select NASCAR88W, then press "INSTALL REPAINT(S), last push OK and you're done.

3. Thank you to Gary Claridge-King for the original textures, all I had to do was make the winglet texture.


Like what you see? Come check us out at our website http://www.vnorthwest.com

Rework by: James Bishop 